{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Info","Trassid","Hydrandid","Kaevud","S6lmed","Sulgeseadmed","Reoveepumplad","Puurkaev_pumpla","Reoveepuhastid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Info","index":0,"n_rows":2,"n_cols":11,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["ID","T88_nr","T88_nimi","Teostaja_nimi","Kontakt","M66distaja","CAD_faili_nimi","M66tkava","M66tmise_kpv","Vald","Asula"]
[1,"TM16065","Rannu reoveepuhasti puhastatud biotiikide ja rekonstrueeritud torustike teostusmõõdistus","Geoweb OÜ","Lutsu 16-17, Tartu","Meelis Võsaste","TM16065_Rannu_RVP_biotiikide_teostus_130117.dgn",500,"2017-01-11","Rannu vald","Rannu alevik"]

{"sheet":"Trassid","index":1,"n_rows":31,"n_cols":10,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
["ID"," Kood","X","Y","Z","L2bim66t","Materjal","Otstarve","Ehitusaasta","M2rkus"]
[1,502,6457895.2649999997,629922.375,45.23,160,"PVC","Tänavatoru",2017]
[1,null,6457892.2920000004,629913.69099999999,44.96]
[2,502,6457892.2920000004,629913.69099999999,44.49,160,"PVC","Tänavatoru",2017]
[2,null,6457895.6430000002,629910.85100000002,44.39,null,null,null,null,"toru ots biotiigis"]
[3,502,6457892.284,629913.696,44.49,160,"PVC","Tänavatoru",2017]
[3,null,6457897.6409999998,629914.54299999995,44.41,null,null,null,null,"toru ots biotiigis"]
[4,502,6457949.1289999997,629886.49199999997,43.42,200,"PVC","Tänavatoru",2017,"toru ots biotiigis"]
[4,null,6457955.0219999999,629884.34299999999,43.25]
[4.5,502,6457955.0219999999,629884.34299999999,43.25,200,"PVC","Tänavatoru",2017]
[4.9000000000000004,null,6457972.0619999999,629878.28899999999,43.16,null,null,null,null,"toru ots biotiigis"]
[5.7,502,6457952.2280000001,629895.87100000004,43.36,200,"PVC","Tänavatoru",2017,"toru ots biotiigis"]
[6.1,null,6457958.0659999996,629893.973,43.25]
[6.5,502,6457958.0659999996,629893.973,43.25,200,"PVC","Tänavatoru",2017]
[7,null,6457976.0609999998,629887.91500000004,43.17,null,null,null,null,"toru ots biotiigis"]
[8,502,6458027.3210000005,629858.33400000003,42.61,200,"PVC","Tänavatoru",2017,"toru ots biotiigis"]
[8,null,6458031.4139999999,629857.01199999999,42.49]
[9,502,6458031.4139999999,629857.01199999999,42.49,200,"PVC","Tänavatoru",2017]
[9,null,6458038.9210000001,629854.31499999994,42.47,null,null,null,null,"toru ots biotiigis"]
[10,502,6458031.0959999999,629867.84,42.69,200,"PVC","Tänavatoru",2017,"toru ots biotiigis"]
[10,null,6458035.1710000001,629866.37800000003,42.5]
[10.5,502,6458035.1710000001,629866.37800000003,42.5,200,"PVC","Tänavatoru",2017]
[10.9,null,6458043.0990000004,629863.04399999999,42.49,null,null,null,null,"toru ots biotiigis"]
[12,502,6458114.2130000005,629821.02500000002,42.6,200,"PVC","Tänavatoru",2017,"toru ots biotiigis"]
[11.7,null,6458111.8940000003,629808.65399999998,42.31]
[13,502,6458111.8940000003,629808.65399999998,42.33,200,"PVC","Tänavatoru",2017]
[12.92,null,6458112.2709999997,629808.04599999997,42.33]
[13,null,6458111.1610000003,629803.321,42.31,null,null,null,null,"heitvee väljalask kraavi"]
[14,502,6458111.8940000003,629808.65399999998,42.31,200,"PVC","Tänavatoru",2017]
[13.86,null,6458111.6940000001,629807.80200000003,42.31]
[14,null,6458110.7019999996,629803.57900000003,42.31]

{"sheet":"Hydrandid","index":2,"n_rows":1,"n_cols":10,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","Maapinna_Z","T2histus","Tyyp","Mark","Toru_l2bim66t","Ehitusaasta","M2rkus"]

{"sheet":"Kaevud","index":3,"n_rows":8,"n_cols":21,"rows_kept":8,"cut":false,"hidden":false,"merged":[]}
["ID"," Kood","X","Y","Maapinna_Z","P6hi","Kaane_l2bim66t","Kaane_materjal","Kaane_tyyp","Kaane_k6rgus","Kaevu_l2bim66t","Kaevu_materjal","Kaevu_tyyp","M2rkus","Ehitusaasta","Toru1","Toru2","Toru3","Toru4","Toru5","Toru6"]
[1,509,6457892.2920000004,629913.69099999999,45.63,44.47,500,"Malm","Kinnine",45.75,"560/500","Plast","Jaotuskaev",null,2017,"44.49 PVC 160","44.49 PVC 160","44.96 PVC 160"]
[2,509,6457895.2649999997,629922.375,46.29,45.32,300,"Malm","Kinnine",46.29,"400/315","Plast","Vaatluskaev",null,2017,"45.23 PVC 160","45.23 PVC 160"]
[3,509,6457958.0659999996,629893.973,44.89,43.35,200,"Plast","Kinnine",45.46,200,"Plast","Vaatluskaev",null,2017,"43.25 PVC 200","43.25 PVC 200"]
[4,509,6457955.0219999999,629884.34299999999,44.89,43.25,200,"Plast","Kinnine",45.42,200,"Plast","Vaatluskaev",null,2017,"43.25 PVC 200","43.25 PVC 200"]
[5,509,6458031.4139999999,629857.01199999999,43.89,42.49,200,"Plast","Kinnine",44.6,200,"Plast","Vaatluskaev",null,2017,"42.49 PVC 200","42.49 PVC 200"]
[6,509,6458035.1710000001,629866.37800000003,43.94,42.5,null,null,null,44.6,200,"Plast","Vaatluskaev",null,2017,"42.50 PVC 200","42.50 PVC 200"]
[7,509,6458111.8940000003,629808.65399999998,43.75,42.31,820,"Plast","Kinnine",42.29,750,"Plast","Proovivõtukaev",null,2017,"42.33 PVC 200","42.31 PVC 200","42.31 PVC 200"]

{"sheet":"S6lmed","index":4,"n_rows":3,"n_cols":11,"rows_kept":3,"cut":false,"hidden":false,"merged":[]}
["ID","Kood","Otstarve","X","Y","K6rgus","Maapinna_Z","Ehitusaasta","M2rkus","Skeemi_nr","L2bim66t"]
[1,516,"põlv",6458112.2709999997,629808.04599999997,42.33,43.75,2017,"käänik 45",null,200]
[2,516,"siiber",6458111.6940000001,629807.80200000003,42.31,43.56,2017,null,null,200]

{"sheet":"Sulgeseadmed","index":5,"n_rows":2,"n_cols":9,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Maapinna_Z","Tyyp","Otstarve","M2rkus","Ehitusaasta"]
[1,6458111.6940000001,629807.80200000003,42.31,43.56,"Siiber","Tänavatoru siiber","DN200",2017]

{"sheet":"Reoveepumplad","index":6,"n_rows":1,"n_cols":24,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Pumpla_nimi","Pumpla_tyyp","Pumpla_v6imsus_m3_d","Pumpla_ehitusaasta","Pumpade_arv","1_pump_pumpamisv6imsus_m3_h","1_pump_t6stek6rgus_m","1_pumba_mark","1_pump_ehitusaasta","2_pump_pumpamisv6imsus_m3_h","2_pump_t6stek6rgus_m","2_pumba_mark","2_pump_ehitusaasta","3_pump_pumpamisv6imsus_m3_h","3_pump_t6stek6rgus_m","3_pumba_mark","3_pump_ehitusaasta","Signalisatsioon","Kaugjuhitav","M2rkus"]

{"sheet":"Puurkaev_pumpla","index":7,"n_rows":1,"n_cols":18,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Puurkaevu_tyyp","Astmelisus","Puurkaevu_nimi","Passi_katastri_number","Puurkaevu_tootlikkus_m3_d","Pumba_t6stek6rgus_m","Pumba_v6imsus","Pumba_tootlikkus_m3_d","Pumpade_arv","Kaugjuhitav","Signalisatsioon","Veet88tlusega","Puurkaevu_ehitusaasta","M2rkus"]

{"sheet":"Reoveepuhastid","index":8,"n_rows":2,"n_cols":20,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Biotiik","Yhtlustusmahuti_x_m3","L2mmastiku_mahuti_x_m3","Aeratsioonimahuti_x_m3","J2relsetiti_x_m2","Mudatihendi_x_m3","Aktiivmudapuhasti_l2bivooluga","Aktiivmudapuhasti_SBR","Nimi","J6udlus","Kaugjuhitav","Septik","Signalisatsioon","Tyyp","Ehitusaasta","M2rkus"]
[1,6458111.1610000003,629803.321,42.31,"jah",null,null,null,null,null,null,null,"Rannu reoveepuhasti",null,null,null,null,null,2017,"heitvee väljalasketoru ots"]