{"text_format":"1","workbook":"xlsx","n_sheets":9,"sheets":["Info","Trassid","Hydrandid","Kaevud","S6lmed","Sulgeseadmed","Reoveepumplad","Puurkaev_pumpla","Reoveepuhastid"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Info","index":0,"n_rows":2,"n_cols":11,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["ID","T88_nr","T88_nimi","Teostaja_nimi","Kontakt","M66distaja","CAD_faili_nimi","M66tkava","M66tmise_kpv","Vald","Asula"]
[1,"GEO5128","Elva aia-ja haljastusjäätmete kompostimisplatsi I etappi teostusmõõdistus","OÜ Maainsener ","Turu tn 34, Tarty","Janis Saks","5128_Elva_kompostiv2ljaku_teostus",0.3888888888888889,"2018-07-25","Elva vald","Kurelaane küla"]

{"sheet":"Trassid","index":1,"n_rows":11,"n_cols":10,"rows_kept":11,"cut":false,"hidden":false,"merged":[]}
["ID"," Kood","X","Y","Z","L2bim66t","Materjal","Otstarve","Ehitusaasta","M2rkus"]
[1,504,6456526.949,640201.94999999995,56.85,315,"PP","Tänavatoru",2018]
[1,504,6456571.1100000003,640160.18599999999,57.06,315,"PP","Tänavatoru",2018]
[2,504,6456571.1100000003,640160.18599999999,57.06,200,"PP","Tänavatoru",2018]
[2,504,6456575.2999999998,640156.38,50.07,200,"PP","Tänavatoru",2018]
[3,504,6456575.2999999998,640156.38,57.12,200,"PP","Tänavatoru",2018]
[3,504,6456589.0700000003,640143.28,57.18,200,"PP","Tänavatoru",2018]
[4,504,6456589.0700000003,640143.28,57.18,200,"PP","Tänavatoru",2018]
[4,504,6456607.1500000004,640162.72,57.29,200,"PP","Tänavatoru",2018]
[5,504,6456589.0700000003,640143.28,57.18,200,"PP","Tänavatoru",2018]
[5,504,6456571.9699999997,640124.05000000005,57.32,200,"PP","Tänavatoru",2018]

{"sheet":"Hydrandid","index":2,"n_rows":1,"n_cols":10,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","Maapinna_Z","T2histus","Tyyp","Mark","Toru_l2bim66t","Ehitusaasta","M2rkus"]

{"sheet":"Kaevud","index":3,"n_rows":7,"n_cols":21,"rows_kept":7,"cut":false,"hidden":false,"merged":[]}
["ID"," Kood","X","Y","Maapinna_Z","P6hi","Kaane_l2bim66t","Kaane_materjal","Kaane_tyyp","Kaane_k6rgus","Kaevu_l2bim66t","Kaevu_materjal","Kaevu_tyyp","M2rkus","Ehitusaasta","Toru1","Toru2","Toru3","Toru4","Toru5","Toru6"]
[1,510,6456526.949,640201.94999999995,58.18,56.78,500,"Metall","Kinnine",58.17,"560/500","Plast",null,null,2018,"56.79 De315 PP","56.85 De315 PP"]
[2,510,6456571.1100000003,640160.18599999999,58.22,56.99,500,"Metall","Kinnine",58.24,"560/500","Plast",null,null,2018,"57.06 De315 PP","57.06 De200 PP"]
[3,510,6456575.2999999998,640156.38,58.19,55.77,640,"Metall","Kinnine",58.19,"5230x1600","klaasplast",null,null,2018,"57.07 De200 PP","57.12 De200 PP",null,"55.94 De160 PVC"]
[4,510,6456589.0700000003,640143.28,58.32,57.13,500,"Metall","Kinnine",58.32,"560/500","Plast",null,null,2018,"57.18 De200 PP","57.18 De200 PP","57.18 De200 PP"]
[5,510,6456607.1500000004,640162.72,58.2,56.57,500,"Metall","Kinnine",58.19,"560/500","Plast",null,null,2018,"57.29 De200 PP"]
[6,510,6456571.9699999997,640124.05000000005,58.13,56.57,500,"Metall","Kinnine",58.12,"560/501","Plast",null,null,2018,"57.32 De200 PP"]

{"sheet":"S6lmed","index":4,"n_rows":1,"n_cols":11,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["ID","Kood","Otstarve","X","Y","K6rgus","Maapinna_Z","Ehitusaasta","M2rkus","Skeemi_nr","L2bim66t"]

{"sheet":"Sulgeseadmed","index":5,"n_rows":2,"n_cols":9,"rows_kept":2,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Maapinna_Z","Tyyp","Otstarve","M2rkus","Ehitusaasta"]
[1,6456572.2599999998,640159.16200000001,57.06,58.22,"Siiber","Tänavatoru siiber",null,2018]

{"sheet":"Reoveepumplad","index":6,"n_rows":1,"n_cols":24,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Pumpla_nimi","Pumpla_tyyp","Pumpla_v6imsus_m3_d","Pumpla_ehitusaasta","Pumpade_arv","1_pump_pumpamisv6imsus_m3_h","1_pump_t6stek6rgus_m","1_pumba_mark","1_pump_ehitusaasta","2_pump_pumpamisv6imsus_m3_h","2_pump_t6stek6rgus_m","2_pumba_mark","2_pump_ehitusaasta","3_pump_pumpamisv6imsus_m3_h","3_pump_t6stek6rgus_m","3_pumba_mark","3_pump_ehitusaasta","Signalisatsioon","Kaugjuhitav","M2rkus"]

{"sheet":"Puurkaev_pumpla","index":7,"n_rows":1,"n_cols":18,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Puurkaevu_tyyp","Astmelisus","Puurkaevu_nimi","Passi_katastri_number","Puurkaevu_tootlikkus_m3_d","Pumba_t6stek6rgus_m","Pumba_v6imsus","Pumba_tootlikkus_m3_d","Pumpade_arv","Kaugjuhitav","Signalisatsioon","Veet88tlusega","Puurkaevu_ehitusaasta","M2rkus"]

{"sheet":"Reoveepuhastid","index":8,"n_rows":1,"n_cols":20,"rows_kept":1,"cut":false,"hidden":false,"merged":[]}
["ID","X","Y","K6rgus","Biotiik","Yhtlustusmahuti_x_m3","L2mmastiku_mahuti_x_m3","Aeratsioonimahuti_x_m3","J2relsetiti_x_m2","Mudatihendi_x_m3","Aktiivmudapuhasti_l2bivooluga","Aktiivmudapuhasti_SBR","Nimi","J6udlus","Kaugjuhitav","Septik","Signalisatsioon","Tyyp","Ehitusaasta","M2rkus"]